## Use of the Tilt-Carrier is only suited to vehicles such as the larger SUV’s, Vans, trucks, caravans and mobile homes which generally have longer wheel bases than cars.

Australian State government transport departments have varying rules that the owner of the Tilt-Carrier must follow and they include:

1. Install the Tilt-Carrier to your vehicle using the Bogie Wheel supplied. See Tilt-Carrier Accessories and Assembly Instructions on this website.
2. Drive sensibly and with safety. Avoid driving over large/sharp undulations and gutters in the roadway.
3. Don't exceed your vehicles tow bar capacity rating.
4. Use a hitch drop/riser if the vehicles hitch mount is too high/low. See Tilt-Carrier Accessories on this website.
5. Use an Anti-Tilt Bracket on the hitch bar to eliminate as much rattle/wobble as possible. See Tilt-Carrier Accessories on this website.
6. Do not ride you wheelchair/mobility scooter/golf cruiser onto or off the Tilt-Carrier and only load/unload while walking alongside.
7. If the Tilt-Carrier & the wheelchair/mobility scooter/golf cruiser sitting on it obstructs the lights and/or number plate (Tail, Indicator & Brake Lights), you will need to install a Light Bar Kit to the Tilt-Carrier. See Tilt-Carrier Accessories on this website.
8. Make sure you install a copy-number plate/identifier to the back of the Tilt-Carrier. The Light Bar Kit has a number plate light and number plate holder.
9. Always tie down your scooter when it is sitting on the Tilt-Carrier. You can do this by using the strong ratchet straps that we can provide. See Tilt-Carrier Accessories on this website.
10. Take extra care when loading and unloading your wheelchair/mobility scooter/golf cruiser. Always look out for traffic. Load/unload from a curb-side raised nature strip if available, to reduce the loading ramp angle.
11. The vehicle's rear overhang with the carrier attached must not exceed 1.2 meters from the vehicle, or 60% of the vehicle's wheelbase, or 3.70m, whichever is lesser. A flag may be required. Check with your local State transport department.
12. When travelling without a wheelchair/mobility scooter/golf cruiser sitting on the Tilt-Carrier, move the Tilt-Carrier to the vertical position and move the Light Bar/Number Plate Holder to face the rear.

**As vehicle types vary, it's up to you to make sure that you comply with the road rules at all times.**